* A supercritical extraction model with decaying extraction kinetics and Cubic Equation of State is presented
* Model parameters are determined through maximum likelihood estimation based on a set of experimental performed at different operating conditions
* The multiple linear regression is used to find correlations between the estimated parameters and operating conditions
* The close fit between the model predictions and experimental data underscores the model's capability to capture the system dynamics